// - - - - - - - - - - - - - - - - - - - - - - - - - - - -
// Configuration for pico-8
// 
// config.txt is read on startup and saved on exit.
// To generate the default config.txt, delete this file.
// 
// - - - - - - - - - - - - - - - - - - - - - - - - - - - -


// :: Video Settings

window_size 640 480 // window width, height
screen_size 1280 720 // screen width, height (stretched to window) 
show_fps 0 // Draw frames per second in the corner


// :: Window Settings

windowed 0 // 1 to start up in windowed mode
window_position -1 -1 // x and y position of window (-1, -1 to let the window manager decide)
frameless 1 // 1 to use a window with no frame
fullscreen_method 2 // 0 maximized window (linux)  1 borderless desktop-sized window  2 hardware fullscreen (warning: erratic behaviour under some drivers)
blit_method 0  // 0 auto  1 software (slower but sometimes more reliable)  2 hardware (can do filtered scaling) 



// :: System Settings

foreground_sleep_ms 4 // number of milliseconds to sleep each frame. Try 10 to conserve battery power

background_sleep_ms 8 // number of milliseconds to sleep each frame when running in the background

sessions 894 // number of times program has been run

// (scancode) hold this key down and left-click to simulate right-click
rmb_key 0 // 0 for none  226 for LALT

// Desktop for saving screenshots etc. Defaults to $HOME/Desktop
desktop_path 

// 1 to allow controller input even when application is in background
read_controllers_in_background 0



// :: Audio Settings (use "volume" for PICO-8)

sound_volume 256 // 0..256
music_volume 256 // 0..256


// :: usually 1024. Try 2048 if you get choppy sound

mix_buffer_size 1024


// :: map scancodes. Format: 44=47,80=89,..  (scancode a, scancode b -- when press a, generates b)
// run the program with -scancodes to determine which scancodes to use
map_scancodes 


use_wget 0 // (Linux) 1 to use wget for downloads instead of libcurl (must be installed)



// :: pico-8 

version 0.2.6b

// audio volume: 0..256 
volume 256


// Location of pico-8's root folder
root_path /mnt/SDCARD/Emus/PICO8/pico/.lexaloffle/pico-8/carts/


// Location of cartridge save data
cdata_path /mnt/SDCARD/Emus/PICO8/pico/.lexaloffle/pico-8/cdata/


// Specify which player index joystick control begins at (0..7)
joystick_index 0


// Treat the first n controllers as if they were a single merged controller
// e.g. merge_joysticks 2 --> P0 gets controllers 0,1, P1 gets controller 2..
merge_joysticks 0


// Custom keyboard scancodes for buttons. player0 0..6, player1 0..5, menu_button, player2 0..5, player3 0..5
button_keys 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 0 

// Play notes as they are plotted in frequency mode
live_notes 0

// iff 1: when using keyboard cursor, snap to closest pixel / map cel
cursor_snap 0

// 0 default  1 dark blue background in code editor  2 black background in code editor   3 gray background in code editor   
gui_theme 0

// scale of screenshots and gifs // 2 means 256x256
screenshot_scale 3
gif_scale 2

// maximum gif length in seconds (0..120; 0 means no gif recording)
gif_len 8

// when 1, reset the recording when pressing ctrl-9 (useful for creating a non-overlapping sequence)
gif_reset_mode 0

// 0 for off. 1 for auto. 2 to allow control of a cart's framerate due to host machine's cpu capacity
host_framerate_control 1

// filter splore cartridges
// 0 off   1 on (exclude cartridge tagged as 'mature' by community)
splore_filter 0

// tab display width (1 ~ 4 spaces)
tab_width 1

// 0 off 1 on: draw tab characters as small vertical lines
draw_tabs 0

// 0 off 1 on: record the current cartridge and editor view every 3 seconds (see [appdata]/activity.log.txt)
record_activity_log 1

// 0 off 1 on: allow F6..F9 (alternative: ctrl 6..9)
allow_function_keys 1

// 0 off 1 on: automatically check for a newer version of a BBS cart each time it is run.
check_for_cart_updates 1

// 0 off 1 on: allow access to hardware GPIO at 0x5f80..0x5fff (might need to sudo pico8)
enable_gpio 1

// hide mouse cursor for n seconds when typing.
auto_hide_mouse_cursor 5

// 0 off 1 on: backup with a new timestamped filename on every run
// normally not needed -- was used for debugging crash-on-run
aggressive_backups 0

// back up cartridge in editor every n minutes when not idle (0 for no periodic backups)
periodic_backups 20

// global screen transformations:
//  129 flip horizontally
//  130 flip vertically
//  133 rotate CW 90 degrees
//  134 rotate CW 180 degrees
//  135 rotate CW 270 degrees
transform_screen 0

// 0 off  > 1: colour to draw pixel grid in the gfx editor at zoom:8 and zoom:4 (16 for black)
gfx_grid_lines 0

// file naming for screenshot / gif / wav captures
// 0 sequential (foo_0.png, foo_1.png)    1 timestamp (foo_20240115_120823.png)
capture_timestamps 0

