#
# this CSV file defines a color template for a binary file.
#
# This file targets:  Mifare Classic mini s20 , 320b, 4 byte UID
# 
# 2018, hiwanz
# block 0
0; 4; DeepPink; Black; UID
4; 1; DeepSkyBlue; Black; BCC
5; 48; White; black; Text
(0*64) + 48; 6; Orange; Black; Key A
(0*64)+ 48+ 6; 3; Red; Black; Access bytes
(0*64)+ 48+ 9; 1; Aquamarine; Black; GDC byte
(0*64) + 48+10; 6; SkyBlue; Black; Key B
# block 1
(1*64); 48; White; black; Text
(1*64) + 48; 6; Orange; Black; Key A
(1*64)+ 48+ 6; 3; Red; Black; Access bytes
(1*64)+ 48+ 9; 1; Aquamarine; Black; GDC byte
(1*64) + 48 +10; 6; SkyBlue; Black; Key B
# block 2
(2*64); 48; White; black; Text
(2*64) + 48; 6; Orange; Black; Key A
(2*64)+ 48+ 6; 3; Red; Black; Access bytes
(2*64)+ 48+ 9; 1; Aquamarine; Black; GDC byte
(2*64) + 48 +10; 6; SkyBlue; Black; Key B
# block 3
(3*64); 48; White; black; Text
(3*64) + 48; 6; Orange; Black; Key A
(3*64)+ 48+ 6; 3; Red; Black; Access bytes
(3*64)+ 48+ 9; 1; Aquamarine; Black; GDC byte
(3*64) + 48 +10; 6; SkyBlue; Black; Key B
# block 4
(4*64); 48; White; black; Text
(4*64) + 48; 6; Orange; Black; Key A
(4*64)+ 48+ 6; 3; Red; Black; Access bytes
(4*64)+ 48+ 9; 1; Aquamarine; Black; GDC byte
(4*64) + 48 +10; 6; SkyBlue; Black; Key B