#
# this CSV file defines a color template for a binary file.
#
# This file targets:   Mifare Classic mini s20 , 320b,  4 byte UID
# 
# 2018, iceman
# block 0
0; 4; Turquoise; DarkGray; UID
4; 1; white; DarkGray; BCC
(0*64) + 48; 6; yellow; DarkGray; Key A
(0*64)+ 48+ 6; 3; darkred; DarkGray; Access bytes
(0*64)+ 48+ 9; 1; Aquamarine; DarkGray; GDC byte
(0*64) + 48+10; 6; blue; DarkGray; Key B
# block 1
(1*64) + 48; 6; yellow; DarkGray; Key A
(1*64)+ 48+ 6; 3; darkred; DarkGray; Access bytes
(1*64)+ 48+ 9; 1; Aquamarine; DarkGray; GDC byte
(1*64) + 48 +10; 6; blue; DarkGray; Key B
# block 2
(2*64) + 48; 6; yellow; DarkGray; Key A
(2*64)+ 48+ 6; 3; darkred; DarkGray; Access bytes
(2*64)+ 48+ 9; 1; Aquamarine; DarkGray; GDC byte
(2*64) + 48 +10; 6; blue; DarkGray; Key B
# block 3
(3*64) + 48; 6; yellow; DarkGray; Key A
(3*64)+ 48+ 6; 3; darkred; DarkGray; Access bytes
(3*64)+ 48+ 9; 1; Aquamarine; DarkGray; GDC byte
(3*64) + 48 +10; 6; blue; DarkGray; Key B
# block 4
(4*64) + 48; 6; yellow; DarkGray; Key A
(4*64)+ 48+ 6; 3; darkred; DarkGray; Access bytes
(4*64)+ 48+ 9; 1; Aquamarine; DarkGray; GDC byte
(4*64) + 48 +10; 6; blue; DarkGray; Key B